|  |
| --- |
| **Challenges:** |
|

|  |
| --- |
| **Challenge 1:** Use the rv.color\_rgb() function to explore using the color LED. Try to find RGB values for the primary and secondary colors.e.g. rv.color\_rgb(255,155,0) will make yellow. |

 |

|  |
| --- |
| **Challenge 2:** Use the text\_at() function to display your name at several locations on the screen. |

 |
|

|  |
| --- |
| **Challenge 3:** Have Rover drive 5 units forward. Use the rv.waypoint\_x() function to read and display Rover’s horizontal position when Rover is finished driving.  |

 |

|  |
| --- |
| **Challenge 4:** Use a While loop to turn on the LED red, then green, then blue each for 1 second until the escape key is pressed.  |

 |

|  |
| --- |
| **Challenges:** |
|

|  |
| --- |
| **Challenge 5:** Have Rover drive 5 units forward. Predict the amount of time for Rover to reach 4 units and read Rover’s position at that time. If the value returned is equal to 4 turn the LED green, if the value returned is less than 4 turn the LED red, and if the value is greater than 4, turn the LED blue.  |

 |

|  |
| --- |
| **Challenge 6:** Have Rover drive on the number line between 0 and 10. While Rover is driving, read its position and control the LED so that the LED displays colors corresponding to the number line diagram below. |

 |
|

|  |
| --- |
| **Challenge 7:** Have Rover drive on the number line between 0 and 10. While Rover is driving, read its position and control the LED so that the LED displays colors corresponding to the number line diagram below. |

 |

|  |
| --- |
| **Challenge 8:** Have Rover drive on the number line between -10 and 10. While Rover is driving, read its position and control the LED so that the LED displays colors corresponding to the description below.* While Rover’s position is less than or equal to zero, the LED is magenta.
* While Rover’s position is greater than 0 and less than 2, the LED is off.
* While Rover’s position is greater than or equal to 2 and less than or equal to 4, the LED is red.
* While Rover’s position is greater than 4 and less than 5, the LED is blue.
* While Rover’s position is greater than or equal to 5 and less than 10, the LED is green.
* While Rover’s position is greater than or equal to 10, the LED is yellow.

 |

 |